|  |  |  |  |
| --- | --- | --- | --- |
| **編號** | **符號** | **顏色** | **意義** |
| **1** | HOT SURFACE | 黃色警告 | heat / fire |
| **2** | Hot Surface Underneath | 黃色警告 | heat / fire |
| **3** | Hot Surface Underneath-2 | 黃色警告 | heat / fire |
| **4** | [ISO P010 - Do Not Touch](http://www.mysafetylabels.com/MSL/ISO-Prohibition-Do-Not-Touch-Safety-Label/SKU-LB-0310.aspx) | 禁止 | heat/ fire |
| **5** | [Do Not Operate Guard Removed Label](http://www.mysafetylabels.com/MSL/ISO-Prohibition-Do-Not-Operate-Safety-Label/SKU-LB-0284.aspx) | 禁止 | guard label |
| **6** | [Do Not Operate With Guard Removed Label](http://www.mysafetylabels.com/MSL/ISO-Prohibition-Do-Not-Operate-Safety-Label/SKU-LB-0285.aspx) | 禁止 | guard label |
| **7** | [ISO P002 No Smoking Label](http://www.mysafetylabels.com/MSL/ISO-Prohibition-No-Smoking-Safety-Label/SKU-LB-0318.aspx) | 禁止 | heat / fire |

|  |  |  |  |
| --- | --- | --- | --- |
| **編號** | **符號** | **顏色** | **意義** |
| **8** | [ISO M006 - Disconnect Mains Plug](http://www.mysafetylabels.com/Safety-Labels/ISO-Label-Disconnect-Mains-Plug/SKU-LB-0460.aspx) | disconnect power | electrical |
| **9** | [Lock Out Electric Power](http://www.mysafetylabels.com/Safety-Labels/ISO-Label-Lock-Out-Electric-Power/SKU-LB-0468.aspx) | lockout electrical power | electrical |
| **10** | [ISO W018 - Automatic Start-up](http://www.mysafetylabels.com/Warning-Labels/ISO-Automatic-Startup-Safety-Label/SKU-LB-0106.aspx) | 黃色警告 | electrical |
| **15** | [Flying Debris And Loud Noise (Symbol) Label](http://www.mysafetylabels.com/Warning-Labels/Flying-Debris-Loud-Noise-Safety-Label/SKU-LB-0236.aspx) | 黃色警告 | environmental |
| **16** | [Loud Noise (with symbol)](http://www.mysafetylabels.com/Warning-Labels/ISO-Triangle-Loud-Noise-Safety-Label/SKU-LB-0242.aspx) | 黃色警告 | environmental |
| **17** | [ISO P019 Do Not Step Label](http://www.mysafetylabels.com/MSL/ISO-Prohibition-Do-Not-Step-Safety-Label/SKU-LB-0248.aspx) | 禁止 | environmental |

|  |  |  |  |
| --- | --- | --- | --- |
| **編號** | **符號** | **顏色** | **意義** |
| **18** | LASER BEAM | 黃色警告 | laser |
| **19** | [ISO 3864-2 Refer Operator'S Manual Label](http://www.mysafetylabels.com/Safety-Labels/ISO-Label-Refer-to-Operators-Manual/SKU-LB-0458.aspx) |  | read manual |
| **20** | [Read Operators Manual Symbol Safety Label](http://www.mysafetylabels.com/labels/read-operators-manual-symbol-mandatory-label/sku-lb-1630.aspx) |  | read manual |
| **21** | [ISO M004 - Wear Eye Protection](http://www.mysafetylabels.com/MSL/Mandatory-Circle-Wear-Eye-Protection-Safety-Label/SKU-LB-0319.aspx) |  | wear eye protection |
| **22** | [ISO M009 - Wear Safety Gloves](http://www.mysafetylabels.com/MSL/Mandatory-Blue-Circle-Wear-Gloves-Safety-Label/SKU-LB-0316.aspx) |  | wear safety gloves |
| **23** | [ISO M003 - Wear Ear Protection](http://www.mysafetylabels.com/MSL/ISO-Mandatory-Safety-Label-Wear-Ear-Protection/SKU-LB-0326.aspx) |  | wear ear protection |

|  |  |  |  |
| --- | --- | --- | --- |
| **編號** | **符號** | **顏色** | **意義** |
| **24** | [ISO M008 - Wear Foot Protection](http://www.mysafetylabels.com/Protective-Equipment-Hazard-Labels/Foot-Protection/SKU-LB-0461.aspx) |  | wear shoes |
| **25** | [Flying Debris And Loud Noise (Symbol) Label](http://www.mysafetylabels.com/Warning-Labels/Flying-Debris-Loud-Noise-Safety-Label/SKU-LB-0236.aspx) | 黃色警告 | flying debris and loud noise |
| **26** | GENERAL WARNING | 黃色警告 | general warning |
| **27** | [ISO P001 - General Prohibition](http://www.mysafetylabels.com/Safety-Labels/ISO-Label-General-Prohibition/SKU-LB-0469.aspx) | 禁止 | general prohibition |
| **28** | [ISO M001 - General Mandatory Action](http://www.mysafetylabels.com/Safety-Labels/ISO-Label-General-Mandatory-Action/SKU-LB-0457.aspx) |  | general mandatory action |
| **29** |  | 禁止 | no access for unauthorized persons |

|  |  |  |  |
| --- | --- | --- | --- |
| **編號** | **符號** | **顏色** | **意義** |
| **30** | [ISO Label - Do Not Obstruct](http://www.mysafetylabels.com/Safety-Labels/ISO-Label-Do-Not-Obstruct/SKU-LB-0484.aspx) | 禁止 | Stay Clear |
| **31** |  | 禁止 |  |
| **32** | [ISO Do Not Stand Here Label](http://www.mysafetylabels.com/Safety-Labels/ISO-Prohibition-Label-Do-Not-Stand-Here/SKU-LB-0481.aspx) | 禁止 | do not step here |
| **33** |  | 禁止 | no maintenance while machine in use |
| **34** | CORROSIVE MATERIAL | 黃色警告 | corrosive material |
| **35** | ELECTRICAL SHOCK | 黃色警告 | electrical shock / electrocution |

|  |  |  |  |
| --- | --- | --- | --- |
| **編號** | **符號** | **顏色** | **意義** |
| **36** | EXplosive Material | 黃色警告 | explosive material |
| **37** | EXPLOSIVE | 黃色警告 | explosion |
| **38** | [Two Person Lift](http://www.mysafetylabels.com/MSL/ISO-Two-Person-Lift-Circle-Safety-Label/SKU-LB-0023.aspx) |  | two person lift |
| **39** | [Do Not Lift With Hook Label](http://www.mysafetylabels.com/MSL/ISO-Do-Not-Lift-Safety-Label/SKU-LB-0024.aspx) | 禁止 | do not lift with hook / no lift point |
| **40** | [Lift Point Label](http://www.mysafetylabels.com/MSL/ISO-Mandatory-Lift-Point-Safety-Label/SKU-LB-0025.aspx) |  | lift point |
| **41** | [Forklift Point](http://www.mysafetylabels.com/MSL/ISO-Mandatory-Forklift-Point-Safety-Label/SKU-LB-0026.aspx) |  | forklift point (right ) |

|  |  |  |  |
| --- | --- | --- | --- |
| **編號** | **符號** | **顏色** | **意義** |
| **42** | [Forklift Point](http://www.mysafetylabels.com/MSL/ISO-Mandatory-Forklift-Point-Safety-Label/SKU-LB-0027.aspx) |  | forklift point (left) |
| **43** | [Center of Gravity  Label](http://www.mysafetylabels.com/MSL/ISO-Mandatory-Center-Of-Gravity-Safety-Label/SKU-LB-0029.aspx) |  |  |
| **44** | [Lifting Hazard](http://www.mysafetylabels.com/Warning-Labels/ISO-Lifting-Hazard-Safety-Label/SKU-LB-0017.aspx) | 黃色警告 | lifting hazard |
| **45** |  | 黃色警告 | cutting of fingers or hand / angled blade |
| **49** | [Cutting Fingers Hand Blade Label](http://www.mysafetylabels.com/Warning-Labels/ISO-Triangle-Safety-Label/SKU-LB-0181.aspx) | 黃色警告 | cutting of fingers or hand curved blade |
| **50** | [Cut or Sever Hazard](http://www.mysafetylabels.com/Warning-Labels/ISO-Cut-Or-Sever-Hazard-Safety-Label/SKU-LB-0193.aspx) | 黃色警告 | cutting of fingers or hand / straight blade |

|  |  |  |  |
| --- | --- | --- | --- |
| **編號** | **符號** | **顏色** | **意義** |
| **51** | [Hand Crush Force Side Label](http://www.mysafetylabels.com/Warning-Labels/ISO-Triangle-Hand-Crush-Safety-Label/SKU-LB-0188.aspx) | 黃色警告 | hand crush and cut / force from above |
| **52** | [Cutting Fingers Hand Blade Label](http://www.mysafetylabels.com/Warning-Labels/Straight-Blades-Cutting-Safety-Label/SKU-LB-0190.aspx) | 黃色警告 | cutting of fingers of hand / straight blades |
| **53** | [ISO W022 - Sharp Points](http://www.mysafetylabels.com/Warning-Labels/Triangle-Sharp-Points-Safety-Label/SKU-LB-0191.aspx) | 黃色警告 | sharp points |
| **54** | CUTTING FINGER-BLADE2 | 黃色警告 | cutting of fingers or hand rotating blade |
| **55** | CUTTING FINGER-BLADE1 | 黃色警告 | cutting of fingers or hand rotating blade |

|  |  |  |  |
| --- | --- | --- | --- |
| **編號** | **符號** | **顏色** | **意義** |
| **56** | [Hand Crush/Rotating Blade (with symbol)](http://www.mysafetylabels.com/Warning-Labels/Hand-Crush-Rotating-Blade-Safety-Label/SKU-LB-0206.aspx) | 黃色警告 | hand crush / rotating blade |
| **57** | [Cutting Of Fingers Or Hand/Rotating Blade Label](http://www.mysafetylabels.com/Warning-Labels/ISO-Triangle-Safety-Label/SKU-LB-0217.aspx) | 黃色警告 | cutting of fingers or hand rotating blade |
| **58** | Cutting of Fingers or Hand | 黃色警告 | cutting of fingers or hand rotating blade |
| **59** | [Cutting of Fingers or Hand/Engine Fan Label](http://www.mysafetylabels.com/Warning-Labels/ISO-Cutting-Of-Fingers-Safety-Label/SKU-LB-0222.aspx) | 黃色警告 | cutting of fingers or hand engine fan |
| **60** | CUTTING FINGER-AUGER | 黃色警告 | cutting of fingers or hand / auger |
| **61** | [Cutting Of Fingers Or Hand/Moving Part Label](http://www.mysafetylabels.com/img/lg/L/Cutting-Hand-ISO-7010-Safety-Label-LB-0229.gif) | 黃色警告 | cutting of fingers or hand moving part |

|  |  |  |  |
| --- | --- | --- | --- |
| **編號** | **符號** | **顏色** | **意義** |
| **62** | [Cutting Of Fingers Or Hand/Rotating Shaft Label](http://www.mysafetylabels.com/Warning-Labels/ISO-Triangle-Safety-Label/SKU-LB-0230.aspx) | 黃色警告 | cutting of fingers or hand / rotating shaft |
| **63** | ENTANGLEMENT-CHAIN | 黃色警告 | hand entanglement / chain drive |
| **64** | [Pinch Point Entanglement Label](http://www.mysafetylabels.com/Warning-Labels/Pinch-Pointentanglement-Safety-Label/SKU-LB-0344.aspx) | 黃色警告 | hand entanglement / belt drive |
| **65** | [Pinch Point/Entanglement](http://www.mysafetylabels.com/Warning-Labels/Pinch-Pointentanglement-Safety-Label/SKU-LB-0347.aspx) | 黃色警告 | hand entanglement / belt drive |
| **66** | [Pinch Point/Entanglement](http://www.mysafetylabels.com/Warning-Labels/Pinch-Pointentanglement-Safety-Label/SKU-LB-0351.aspx) | 黃色警告 | hand entanglement / belt drive |

|  |  |  |  |
| --- | --- | --- | --- |
| **編號** | **符號** | **顏色** | **意義** |
| **67** | [Pinch Point/Entanglement](http://www.mysafetylabels.com/Warning-Labels/ISO-Triangle-Pinch-Pointentanglement/SKU-LB-0355.aspx) | 黃色警告 | hand entanglement / drawing in rollers |
| **68** | ENTANGMENT-PINCH POINT-3 | 黃色警告 | hand abrasion |
| **69** | [Pinch Point/Entanglement](http://www.mysafetylabels.com/Warning-Labels/Pinch-Pointentanglement-Safety-Label/SKU-LB-0364.aspx) | 黃色警告 | hand entanglement / rollers |
| **70** |  | 黃色警告 | hand crush / robot |
| **71** | [ISO W015-Body Crush / Force Above Label](http://www.mysafetylabels.com/Warning-Labels/ISO-Body-Crush-Force-Safety-Label/SKU-LB-0163.aspx) | 黃色警告 | body crush / force from above |
| **72** | BODY CRUSH | 黃色警告 | body crush / force from side |
| **73** | KICKBACK | 黃色警告 | body impact / |

|  |  |  |  |
| --- | --- | --- | --- |
| **編號** | **符號** | **顏色** | **意義** |
| **74** | [Pinch Point Entanglement Label](http://www.mysafetylabels.com/Warning-Labels/Pinch-Pointentanglement-Safety-Label/SKU-LB-0366.aspx) | 黃色警告 | hand entanglement / rollers |
| **75** | [Pinch Point/Entanglement](http://www.mysafetylabels.com/Warning-Labels/Pinch-Pointentanglement-Safety-Label/SKU-LB-0370.aspx) | 黃色警告 | hand entanglement / rollers |
| **76** | [Pinch Point Entanglement Label](http://www.mysafetylabels.com/Warning-Labels/Pinch-Pointentanglement-Safety-Label/SKU-LB-0372.aspx) | 黃色警告 | hand entanglement / rollers |
| **77** | Entanglement-PINCH POINT | 黃色警告 | hand crush / roller pinch point |
| **78** | ENTANGMENT-PINCH POINT-2 | 黃色警告 | arm or body entanglement / rollers |
| **79** | [Symbol Rotating Shaft](http://www.mysafetylabels.com/Warning-Labels/ISO-Symbol-Rotating-Shaft-Safety-Label/SKU-LB-0380.aspx) | 黃色警告 | arm entanglement / roller shaft |

|  |  |  |  |
| --- | --- | --- | --- |
| **編號** | **符號** | **顏色** | **意義** |
| **80** | [Symbol Rotating Shaft](http://www.mysafetylabels.com/Warning-Labels/ISO-Symbol-Rotating-Shaft-Safety-Label/SKU-LB-0382.aspx) | 黃色警告 | arm entanglement / roller or shaft |
| **81** | DRAW IN CRUSH | 黃色警告 | entanglement / rotating shaft |
| **82** | [Lock-Out In De-Energized State Symbol Label](http://www.mysafetylabels.com/labels/lock-out-in-de-energized-state-mandatory-label/sku-lb-1634.aspx) |  | lock out in de-energized state |
| **83** | [ISO W006 Strong Magnetic Field Label](http://www.mysafetylabels.com/Warning-Labels/ISO-Strong-Magnetic-Field-Safety-Label/SKU-LB-0095.aspx) | 黃色警告 | strong magnetic field |
| **84** | UV LIGHT | 黃色警告 | UV light |
| **85** | [Non-Ionizing Radiation Electromagnetic Hazard Label](http://www.mysafetylabels.com/Warning-Labels/Radiation-Electromagnetic-Hazard-Label/SKU-LB-0100.aspx) | 黃色警告 | non-ionizing radiation |

|  |  |  |  |
| --- | --- | --- | --- |
| **編號** | **符號** | **顏色** | **意義** |
| **86** | SKIN PUNCTURE-AIR PRESSURE | 黃色警告 | skin puncture / pressurized air jet |
| **87** | SKIN PUNCTURE-HYDRAULIC | 黃色警告 | skin puncture / hydraulic line |
| **88** | [Explosion (with symbol)](http://www.mysafetylabels.com/Warning-Labels/ISO-Triangle-Explosion-Safety-Label/SKU-LB-0254.aspx) | 黃色警告 | explosion |
| **89** | EXplosive Material | 黃色警告 | explosion / release of pressure |
| **90** | [ISO W024-Hand Crush/Force From Above Label](http://www.mysafetylabels.com/Warning-Labels/ISO-Hand-Crush-Force-Safety-Label/SKU-LB-0119.aspx) | 黃色警告 | hand crush / force from above |
| **91** | HAND CRUSH FROM ABOVE-HEAVEY | 黃色警告 | hand crush / force from above |
| **92** | HAND CRUSH FROM ABOVE | 黃色警告 | hard crush / force from above |

|  |  |  |  |
| --- | --- | --- | --- |
| **編號** | **符號** | **顏色** | **意義** |
| **93** | [Hand Crush / Pinch Point Label (Symbol)](http://www.mysafetylabels.com/Warning-Labels/Hand-Crush-Pinch-Point-Safety-Label/SKU-LB-0142.aspx) | 黃色警告 | hand crush / pinch point |
| **94** | [Hand Crush Force Side Label](http://www.mysafetylabels.com/Warning-Labels/Label-Hand-Crush-Force-From-Side/SKU-LB-0145.aspx) | 黃色警告 | hand crush / force from side |
| **95** | hand-crush | 黃色警告 | hand crush / force from two sides |
| **96** | [Hand Crush Force Side Label](http://www.mysafetylabels.com/Warning-Labels/ISO-Triangle-Safety-Label/SKU-LB-0155.aspx) | 黃色警告 | hand crush / force from above |
|  |  |  |  |
|  |  |  |  |